# Customer: Date：2021-02-5

**SPECIFICATION & Quotation**

**1、 AIR hoist**

Model： ACH2004S

Unit Price： **50000USD**

Capacity（SWL）： 20T

Lift Height： 12m

work pressure： 4-6 Bar

Chain type： Link Chain

Chain falls: 4 Hook type： with safety latch

Lift speed(no load)： 1.4 meters/min

Lift speed(full load)： 0.7meters/min

AIR consumption： 5.5m³/min

Air trolley

Track width range（H beam） 250-300mm

Traversing speed： 5m/min

Standard Features： Stepless speed regulation/simple and convenient operation/suitable for high temperature, humidity, dust, explosives, etc. Additional features: the above products have automatic overload protection (to prevent overload conditions), limit protection and air cut protection.

# 2、CONTROL

Price： Included

Type： A type Push button Remote Hand Control

**3、 AIR FILTRATION**

Price： Included

Type： AC4000-04

# 4、 AIR PIPE（Spiral Pipe）

Price： Included

Type： Stretch length 9M

DOCUMENTATION Instructions. Instruction Manual (including installation, use, maintenance, lubrication parts list and exploded views).