**Tender/Proposal Detail**

|  |  |  |  |
| --- | --- | --- | --- |
| Tender/Proposal ID : | 515277 | Invitation Reference No. : | 36.091.007.09.52.401.0822.2020 |
| Closing Date and Time : | 21-Dec-2020 11:00 | Opening Date and Time : | 21-Dec-2020 11:00 |
| Procuring Entity : | Chittagong Urea Fertilizer Limited (Commercial) | | |
| Brief : | Procurement of Chain Block, Anchor Shackle & Clamp. | | |

**Technical Specifications and Compliance of Goods and related services (Form e-PG3-4)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No** | **Description of Item** | **Unit** | **Quantity** | **Details Technical Specification and Standard Offered** |
| 1 | Chain Block (CK Type) Capacity: 01 Ton, Standard lift: 3 Miter Column of Load Chain: 01, Load Chain Dia: 6mm Proof load: 1.5 Tons, Head room "H" : 306mm Hook opening "C" : 45mm Pull to lift Rated Load: 304N, Net weight: 10.5 Kg. Brand: KYOTO, Japan or Exact Equivalent. | Nos | 30 | 24 USD/unit |
| 2 | Chain Block (CK Type) Capacity: 02 Ton, Standard lift: 3 Miter Column of Load Chain: 01, Load Chain Dia: 8mm Proof load: 3 Tons, Head room "H" : 444mm Hook opening "C" : 52mm Pull to lift Rated Load: 457N, Net weight: 16.2 Kg. Brand: KYOTO, Japan or Exact Equivalent. | Nos | 30 | 34 USD/unit |
| 3 | Chain Block (CK Type) Capacity: 03 Tons, Standard lift: 3 Miter Column of Load Chain: 02, Load Chain Dia: 8mm Proof load: 4.5 Tons, Head room "H" : 520mm Hook opening "C" : 67mm Pull to lift Rated Load: 390N, Net weight: 22.0 Kg. Brand: KYOTO, Japan or Exact Equivalent. | Nos | 30 | 46 USD/unit |
| 4 | Chain Block (CK Type) Capacity: 05 Tons, Standard lift: 5 Miter Column of Load Chain: 02, Load Chain Dia: 10mm Proof load: 7.5 Tons, Head room "H" : 616mm Hook opening "C" : 78mm Pull to lift Rated Load: 420N, Net weight: 36.0 Kg. Brand: KYOTO, Japan or Exact Equivalent. | Nos | 20 | 80 USD/unit |
| 5 | Chain Block (CK Type) Capacity: 10 Tons, Standard lift: 7 Miter Column of Load Chain: 04, Load Chain Dia: 10mm Proof load: 15 Tons, Net weight: 67.0 Kg. Brand: KYOTO, Japan or Exact Equivalent. | Nos | 5 | 167 USD/unit |
| 6 | Anchor Shackle Size: 3/8" × 7/16 Material: Hot dipped galvanized steel. Type: Standard Screw Pin, Safety Factor: 6:1 Capacity: WLL embossed on each Shackle. Capacity: 01 Ton. | Nos | 30 | n/a |
| 7 | Anchor Shackle Size: 7/16 × 1/2" Material: Hot dipped galvanized steel. Type: Standard Screw Pin, Safety Factor: 6:1 Capacity: WLL embossed on each Shackle. Capacity: 02 Tons. | Nos | 30 | n/a |
| 8 | Anchor Shackle Size: 3/4" × 7/8" Material: Hot dipped galvanized steel. Type: Standard Screw Pin, Safety Factor: 6:1 Capacity: WLL embossed on each Shackle. Capacity: 4.75 Tons. | Nos | 20 | n/a |
| 9 | Clamp (Fixed) Size: 1.5" (For 48mm Pipe) Material: CS (Galv.), As per sample. | Nos | 200 | Pls confirm it is forged or pressed fixed couple, it will be appreciated if you have weight and photos |
| 10 | Clamp (Universal) Size: 1.5" (For 48mm Pipe) Material: CS (Galv.), As per sample. | Nos | 800 | Pls confirm it is forged or pressed swivel couple, it will be appreciated if you have weight and photos |