**Technical specification**

* Manual chain ( worm ) hoist stationary
* The lifting height of the chain hoist should be 6 meters, the total length of the chain shoud be 12 meters.
* Application area general industry + 40 degrees / open areas
* Air humidity 65% - 70%
* GOST 28408-89 or appropriate standard
* Operating temperature of hoists. – 10 / + 50



