|  |  |  |
| --- | --- | --- |
| **Make, Model, Country of Manufacture:** |  | **Offered Specs** |
| Driving Position | Pedestrian |  |
| Lift capacity, kg | 1500-2000 kg  |  |
| Load Center | 500 - 600 mm |  |
| Wheel base | 1250 – 1300mm  |  |
| **Dimensions** |  |  |
| Lifting Height |  4500-5500mm  |  |
| Ground clearance under mast, mm | 30 - 40mm |  |
| Overall length | 1500-1900 mm |  |
| Overall Width | 750-800 mm |  |
| Turning radius mm | 1400-1600mm |  |
| **Forks** |  |  |
|  length, mm | 1000 - 1200 mm |  |
| width, mm  | 150- 200mm |  |
| **Battery** |  |  |
| Electric charger  | Suitable for integral battery |  |
| Battery power | Battery operated |  |
| **Performance** |  |  |
| Travel Speed Loaded / un-loaded | 5 – 8 Km/h |  |
| Service Break | Electromagnetic |  |
| Parking Break | Handle Release |  |
| **Warranty and Post Sales Services Information:** | 1 year after commissioning |  |