|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Item Description** | **Specifications** | **Unit** | **Qty** | **Unit Price** |
| 1. **1**
 | Round lifting slings 5 ton straight pull | Round, hard wearing polyester, 5000kg, 2M length | Pc  | 2 |  |
| 1. **2**
 | Webbing sling 5 ton straight pull | Flat, 150mm width and 3m length, 100% polyester or equivalent, 5100kg  | Pc | 2 |  |
| 1. **3**
 | Round lifting slings 20 ton | Round, hard wearing polyester, 20000kg, 5M length | Pc | 2 |  |
| 1. **4**
 | Webbing sling 10 ton  | Flat, 150mm width and 4m length, 100% polyester or equivalent, 10100kg  | Pc | 2 |  |
| 1. **5**
 | Chain block 2 ton  | * High quality heavy duty
* Standard lift: 3m
* Load chain fall: 1
* Dynamic load: 30KN
* Chain pull to lift full load: 335N
* Load chain diameter: 8x24mm
 | Pc | 1 |  |
| 1. **6**
 | Chain block 5 ton  | Heavy Duty Model, Light Weight, Standard lift: 3m Load **chain** fall: 2 Dynamic load: 75KN **Chain** pull to lift full load: 360N Load **chain** diameter: 9x27mm | Pc | 1 |  |
| 1. **7**
 | Chain block 10 ton | - Capacity (ton): 10 ;- Standard Lifting Height (m): 3- Running Test Load (ton): 15;- Chain fall: 4;- Chain Dia (mm): 10;- Effort to required to lift max.(n): 382;- Net Weight(kg): 75.7 | Pc | 2 |  |
| 1. **8**
 | Ratchet buckles 12 ton | Attribute Zinc plated steel 1”x 4 7/16” | Pc | 2 |  |
| 1. **9**
 | Ratchet buckles 12 ton | Attribute Stainless steel 1”x 4 7/16” | Pc | 2 |  |
| 1. **10**
 | Lever hoist 6 ton | https://www.mcmaster.com/mvD/Contents/gfx/ImageCache/316/3162t511p1-1657902704-p9@1x_637934815699143708.png?ver=ImageNotFoundSteel, Compact heavy duty, 6ton, clearance between 5-10” | Pc | 1 |  |
| 1. **11**
 | Lever hoist 3 ton | Steel, Compact heavy duty, 3ton, clearance between 5-10” | Pc | 1 |  |
| 1. **12**
 | Lever hoist 2 ton | Steel, Compact heavy duty, 2ton, clearance between 5-10” | Pc | 1 |  |
| 1. **31**
 | Chain sling SWL 10 ton  | Grade 80 Steel 4-Leg Chain Sling with Grab Hooks, ASME B30.9, OSHA Compliant | Pc | 2 |  |
| 1. **32**
 | Chain sling SWL 0-45 14 ton  | Grade 80 Steel 4-Leg Chain Sling with Grab Hooks, ASME B30.9, OSHA Compliant | Pc | 2 |  |
| 1. **33**
 | Chain sling SWL 0-45 39 ton  | Grade 80 Steel 4-Leg Chain Sling with Grab Hooks, ASME B30.9, OSHA Compliant | Set  | 2 |  |