|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Item Description** | **Specifications** | **Unit** | **Qty** | **Unit Price** |
| 1. **1** | Round lifting slings 5 ton straight pull | Round, hard wearing polyester, 5000kg, 2M length | Pc | 2 |  |
| 1. **2** | Webbing sling 5 ton straight pull | Flat, 150mm width and 3m length, 100% polyester or equivalent, 5100kg | Pc | 2 |  |
| 1. **3** | Round lifting slings 20 ton | Round, hard wearing polyester, 20000kg, 5M length | Pc | 2 |  |
| 1. **4** | Webbing sling 10 ton | Flat, 150mm width and 4m length, 100% polyester or equivalent, 10100kg | Pc | 2 |  |
| 1. **5** | Chain block 2 ton | * High quality heavy duty * Standard lift: 3m * Load chain fall: 1 * Dynamic load: 30KN * Chain pull to lift full load: 335N * Load chain diameter: 8x24mm | Pc | 1 |  |
| 1. **6** | Chain block 5 ton | Heavy Duty Model, Light Weight,  Standard lift: 3m  Load **chain** fall: 2  Dynamic load: 75KN  **Chain** pull to lift full load: 360N Load **chain** diameter: 9x27mm | Pc | 1 |  |
| 1. **7** | Chain block 10 ton | - Capacity (ton): 10 ;  - Standard Lifting Height (m): 3  - Running Test Load (ton): 15;  - Chain fall: 4;  - Chain Dia (mm): 10;  - Effort to required to lift max.(n): 382;  - Net Weight(kg): 75.7 | Pc | 2 |  |
| 1. **8** | Ratchet buckles 12 ton | Attribute Zinc plated steel 1”x 4 7/16” | Pc | 2 |  |
| 1. **9** | Ratchet buckles 12 ton | Attribute Stainless steel 1”x 4 7/16” | Pc | 2 |  |
| 1. **10** | Lever hoist 6 ton | https://www.mcmaster.com/mvD/Contents/gfx/ImageCache/316/3162t511p1-1657902704-p9@1x_637934815699143708.png?ver=ImageNotFoundSteel, Compact heavy duty, 6ton, clearance between 5-10” | Pc | 1 |  |
| 1. **11** | Lever hoist 3 ton | Steel, Compact heavy duty, 3ton, clearance between 5-10” | Pc | 1 |  |
| 1. **12** | Lever hoist 2 ton | Steel, Compact heavy duty, 2ton, clearance between 5-10” | Pc | 1 |  |
| 1. **31** | Chain sling SWL 10 ton | Grade 80 Steel 4-Leg Chain Sling with Grab Hooks, ASME B30.9, OSHA Compliant | Pc | 2 |  |
| 1. **32** | Chain sling SWL 0-45 14 ton | Grade 80 Steel 4-Leg Chain Sling with Grab Hooks, ASME B30.9, OSHA Compliant | Pc | 2 |  |
| 1. **33** | Chain sling SWL 0-45 39 ton | Grade 80 Steel 4-Leg Chain Sling with Grab Hooks, ASME B30.9, OSHA Compliant | Set | 2 |  |