Compliance Statement- **Hydraulic Hand Trolley**

|  |  |
| --- | --- |
| **Our requirements** | **Your Offer** |
| **Hydroid Hand Trolley** with all standard and additional accessories as per specification below:   1. Specification: 2. Model: To be mentioned 3. Capacity(Minimum): 2Ton (2000kg) 4. Maximum Fork Height (From ground to upper surface of work) : ≥190mm 5. Minimum Fork Height (From ground to upper surface of work) : ≤80mm 6. Fork Dimension:   1)Length: 1200-1400mm  2) Width: 150-160mm  3)Distance between Two forks: 500-540mm(Centre to Centre)  4) Thickness of fork sheet material: ≥3.5mm  f. Size of roller : To be mentioned  g. Steering Wheel Diameter: To be mentioned  h. Wheel Material : To be mentioned   1. Country of Origin, Assembly & Shipment: Group-B 2. **Condition**: 3. All Standard attachment and accessories must be supplied with trollies. 4. Trail run to be done by the supplier. 5. 1 x Operator & 1 x Maintenance Manual in English Must be supplied with machine 6. Must provided warranty for 01(one) year after acceptance. 7. Bidder should submit original leaflet/Brochure with the offer | **Hydroid Hand Trolley, RAMHOIST** with all standard and additional accessories as per specification below:   1. Specification: 2. Model: **HPT02A** 3. Capacity(Minimum): **2Ton (2000kg)** 4. Maximum Fork Height (From ground to upper surface of work) : ≥ **190**  mm 5. Minimum Fork Height (From ground to upper surface of work) : ≤ **80** mm 6. Fork Dimension:   1)Length: **1220**mm  2) Width: **150** mm  3)Distance between Two forks: **550**mm (Centre to Centre)  4) Thickness of fork sheet material:  ≥ **3.5** mm (Actual is 3.75mm)  f. Size of roller : To be mentioned  g. Steering Wheel Diameter: **φ180\*50**  h. Wheel Material : **Nylon wheel**   1. Country of Origin, Assembly & Shipment: **China** 2. **Condition**: 3. All Standard attachment and accessories must be supplied with trollies. **ok** 4. Trail run to be done by the supplier. **?** 5. 1 x Operator & 1 x Maintenance Manual in English Must be supplied with machine **ok** 6. Must provided warranty for 01(one) year after acceptance. **ok** 7. Bidder should submit original leaflet/Brochure with the offer **?** |