Compliance Statement- **Hydraulic Hand Trolley**

|  |  |
| --- | --- |
| **Our requirements**  | **Your Offer**  |
| **Hydroid Hand Trolley** with all standard and additional accessories as per specification below: 1. Specification:
2. Model: To be mentioned
3. Capacity(Minimum): 2Ton (2000kg)
4. Maximum Fork Height (From ground to upper surface of work) : ≥190mm
5. Minimum Fork Height (From ground to upper surface of work) : ≤80mm
6. Fork Dimension:

1)Length: 1200-1400mm2) Width: 150-160mm3)Distance between Two forks: 500-540mm(Centre to Centre) 4) Thickness of fork sheet material: ≥3.5mm f. Size of roller : To be mentioned  g. Steering Wheel Diameter: To be mentioned  h. Wheel Material : To be mentioned1. Country of Origin, Assembly & Shipment: Group-B
2. **Condition**:
3. All Standard attachment and accessories must be supplied with trollies.
4. Trail run to be done by the supplier.
5. 1 x Operator & 1 x Maintenance Manual in English Must be supplied with machine
6. Must provided warranty for 01(one) year after acceptance.
7. Bidder should submit original leaflet/Brochure with the offer
 | **Hydroid Hand Trolley, RAMHOIST** with all standard and additional accessories as per specification below: 1. Specification:
2. Model: **HPT02A**
3. Capacity(Minimum): **2Ton (2000kg)**
4. Maximum Fork Height (From ground to upper surface of work) : ≥ **190**  mm
5. Minimum Fork Height (From ground to upper surface of work) : ≤ **80** mm
6. Fork Dimension:

1)Length: **1220**mm2) Width: **150** mm3)Distance between Two forks: **550**mm (Centre to Centre)  4) Thickness of fork sheet material:  ≥ **3.5** mm (Actual is 3.75mm) f. Size of roller : To be mentioned  g. Steering Wheel Diameter: **φ180\*50** h. Wheel Material : **Nylon wheel**1. Country of Origin, Assembly & Shipment: **China**
2. **Condition**:
3. All Standard attachment and accessories must be supplied with trollies. **ok**
4. Trail run to be done by the supplier. **?**
5. 1 x Operator & 1 x Maintenance Manual in English Must be supplied with machine **ok**
6. Must provided warranty for 01(one) year after acceptance. **ok**
7. Bidder should submit original leaflet/Brochure with the offer **?**
 |