**TECHNICAL SPECFICATION FOR PORC OF HYDRAULIC HAND PALLET TRUCK (CAP: 3000 KG), QTY-09 EA**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Ser No** | **Nomenclature** | **Qty** | **Country of Origin** | **Remarks** |
| 1 | **HYDRAULIC HAND PALLET TRUCK****(CAP: 3000 KG)****Technical Feature:** 1. Brand: To be mention
2. Model: To be mention
3. Capacity: 3000 kg
4. Operating System: Manual
5. Fork height (Max & Min): 200 to 115 mm
6. Fork dimension (H x L x W): Not less than 1150 x 175 x 45 mm
7. Overall dimension (H x L x W): Not less than 1220 x 1510 x 520 mm
 | 09 Ea | To be mention |  |