**Technical Specifications and Compliance of Goods and related services (Form e-PG3-4)**

|  |  |  |  |
| --- | --- | --- | --- |
| Tender/Proposal ID : | **790558** | Invitation Reference No. : | LP-0065/PM/MTS/0505 |
| Closing Date and Time : | 13-Mar-2023 at 11:00 Hrs. | Opening Date and Time : | 13-Mar-2023 at 11:00 Hrs. |
| Procuring Entity : |  |
| Brief : | **Chain Block, Anchor, Shackle & Slings - 35 (Thirty five) items.** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Name of Goods** | **Detailed Technical Specification and Standards required** | **Unit** | **QTY.** | **Full Detailed Technical Specifications and Standards offered** |
| 1 | Chain Block (CK Type) | Chain Block (CK Type)Capacity : 1 TonStandard Lift : 3 meterColumn of load Chain : 1Load Chain Dia : 6 mmProof Load : 1.5 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **15** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 2 | Chain Block (CK Type) | Chain Block (CK Type)Capacity : 1 TonStandard Lift : 5 meter.Column of load Chain : 1Load Chain Dia : 6 mmProof Load : 1.5 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **5** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 3 | Chain Block (CK Type) | Chain Block (CK Type)Capacity : 2 TonStandard Lift : 3 meter.Column of load Chain : 1,Load Chain Dia : 6 mmProof Load : 3.0 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **15** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 4 | Chain Block (CK Type) | Chain Block (CK Type)Capacity : 2 TonStandard Lift : 5 meter.Column of load Chain : 1Load Chain Dia : 6 mmProof Load : 3.0 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **5** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 5 | Chain Block (CK Type) | Chain Block (CK Type)Capacity : 3 TonStandard Lift : 3 meter.Column of load Chain : 1Load Chain Dia : 8 mmProof Load : 4.5 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **10** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 6 | Chain Block (CK Type) | Chain Block (CK Type),Capacity : 5 TonStandard Lift : 5 meter.Column of load Chain : 2Load Chain Dia : 10 mmProof Load : 7.5 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **4** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 7 | Chain Block (CK Type) | Chain Block (CK Type)Capacity : 10 TonStandard Lift : 7 meter.Column of load Chain : 4Load Chain Dia : 10 mmProof Load : 15 TonPreferred Brand: PULLMASTER II, Kyoto or Equivalent. | **Nos.** | **2** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 8 | Lever Chain Hoist | Lever Chain Hoist,Capacity : 01 (one) TonPreferred Brand: Kyoto, Japan or Equivalent | **Nos.** | **2** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 9 | Lever Chain Hoist | Lever Chain Hoist,Capacity: 02 (Two) TonPreferred Brand: Kyoto, Japan or Equivalent  | **Nos.** | **2** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 10 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 7/16''Length : 2 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 11 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 7/16''Length : 3 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 12 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : ½''Length : 2 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 13 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : ½''Length : 3 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 14 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : ½''Length : 5 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 15 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 5/8 ''Length : 2 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 16 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 5/8 ''Length : 3 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 17 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 5/8 ''Length : 5 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 18 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : ¾''Length : 2 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 19 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : ¾''Length : 3 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 20 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : ¾''Length : 5 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 21 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 1''Length : 2 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 22 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 1''Length : 3 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 23 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter :1''Length : 5 meter | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 24 | Single Leg Wire Rope Slings (Soft Eye Machine Swaged) | Single Leg Wire Rope Slings (Soft Eye Machine Swaged),6 x 19 IWRC Stainless Steel (Type 304),Diameter : 1 ''Length : 10 meter | **Pcs.** | **4** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 25 | Anchor Shackle, | Anchor Shackle, Material: Hot Dipped Galvanized Steel,Type : Standard Screw Pin,Safety Factor = 6:1Capacity: WLL embossed on each shackle Capacity : 1 Ton. | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 26 | Anchor Shackle, | Anchor Shackle, Material: Hot Dipped Galvanized Steel, Type : Standard Screw Pin, Safety Factor = 6:1Capacity: WLL embossed on each shackle Capacity : 2 Ton. | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 27 | Anchor Shackle, | Anchor Shackle, Material: Hot Dipped Galvanized Steel, Type : Standard Screw Pin, Safety Factor = 6:1Capacity: WLL embossed on each shackle Capacity : 3 Ton. | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 28 | Anchor Shackle, | Anchor Shackle, Material: Hot Dipped Galvanized Steel, Type : Standard Screw Pin, Safety Factor = 6:1, Capacity: WLL embossed on each shackle Capacity : 5 Ton. | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 29 | Anchor Shackle, | Anchor Shackle, Material: Hot Dipped Galvanized Steel, Type : Standard Screw Pin, Safety Factor = 6:1, Capacity: WLL embossed on each shackle Capacity : 10 Ton. | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 30 | Nylon Plain Eye & Eye Sling, | Nylon Plain Eye & Eye Sling, 2 (Two) Ply Sling,Sling width : 1''Length : 2´ (Two feet) | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 31 | Nylon Plain Eye & Eye Sling, | Nylon Plain Eye & Eye Sling,2 (Two) Ply Sling,Sling width : 1''Length : 4´ (Four feet) | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 32 | Nylon Plain Eye & Eye Sling, | Nylon Plain Eye & Eye Sling, 2 (Two) Ply Sling,Sling width : 2''Length : 4´ (Four feet) | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 33 | Nylon Plain Eye & Eye Sling, | Nylon Plain Eye & Eye Sling, 2 (Two) Ply Sling,Sling width : 2''Length : 6´ (Six feet) | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 34 | Nylon Plain Eye & Eye Sling, | Nylon Plain Eye & Eye Sling, 3 (Three) Ply Sling,Sling width : 3''Length : 8´ (Eight feet) | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |
| 35 | Nylon Plain Eye & Eye Sling, | Nylon Plain Eye & Eye Sling, 3 (Three) Ply Sling, Sling width : 3'', Length : 10´ (ten feet) | **Pcs.** | **8** | Name of the Manufacturer: **To be mention please.**Brand Name: **To be mention please.**Model No: **To be mention please.**Country of Origin: **To be mention please.**Country of Assemble: **To be mention please.****Details Specification:****To be mention please.** |

**N.B.**

a) Manufacturer name and country of origin must be mentioned in the offer.

b) Manufacturer must have 05 (Five) years experience of manufacturing such kind of product.

c) Manufacturer printed product catalogue/brochure in English language must be submitted along with the offer.

d) Preferred Country of origin: JAPAN, Germany, France, CANADA, and UK or Equivalent

f) Manufacturer’s must have ISO/CE Standard Certificate.